{Data points NPTS}{3000}
{Sampling period DT (sec)}{0.0200}
{Record Sequence Number}{1025}
{Earthquake Name}{Northridge-01}
{YEAR}{1994}
{Station Name}{Lancaster - Fox Airfield Grnd}
{Earthquake Magnitude}{6.69}
{Mechanism Based on Rake Angle}{2}
{Hypocenter Latitude (deg)}{34.2057}
{Hypocenter Longitude (deg)}{-118.5539}
{Hypocenter Depth (km)}{17.5}
{EpiD (km)}{67.04}
{HypD (km)}{69.28}
{Joyner-Boore Dist. (km)}{51.88}
{Campbell R Dist. (km)}{52.12}
{RmsD (km)}{61.80}
{ClstD (km)}{52.12}
{GMX's C1}{I}
{GMX's C2}{H}
{GMX's C3}{D}
{Campbell's GEOCODE}{A}
{Preferred NEHRP Based on Vs30}{D}
{Preferred Vs30 (m/s)}{271.4}
{Station Latitude}{34.7390}
{Station Longitude}{-118.2140}
{File Name (Horizontal 1)}{NORTHR/LAN090}
{File Name (Horizontal 2)}{NORTHR/LAN360}
{File Name (Vertical)}{NORTHR/LAN-UP}
{HP-H1 (Hz)}{0.150}
{HP-H2 (Hz)}{0.150}
{LP-H1 (Hz)}{25.000}
{LP-H2 (Hz)}{25.000}
{PGA (g)}{0.0737}
{PGV (cm/sec)}{6.19}
{PGD (cm)}{1.38}
