{Data points NPTS}{1800}
{Sampling period DT (sec)}{0.0200}
{Record Sequence Number}{829}
{Earthquake Name}{Cape Mendocino}
{YEAR}{1992}
{Station Name}{Rio Dell Overpass - FF}
{Earthquake Magnitude}{7.01}
{Mechanism Based on Rake Angle}{2}
{Hypocenter Latitude (deg)}{40.3338}
{Hypocenter Longitude (deg)}{-124.2294}
{Hypocenter Depth (km)}{9.6}
{EpiD (km)}{22.64}
{HypD (km)}{24.55}
{Joyner-Boore Dist. (km)}{7.88}
{Campbell R Dist. (km)}{14.33}
{RmsD (km)}{25.10}
{ClstD (km)}{14.33}
{GMX's C1}{I}
{GMX's C2}{H}
{GMX's C3}{C}
{Campbell's GEOCODE}{A}
{Preferred NEHRP Based on Vs30}{D}
{Preferred Vs30 (m/s)}{311.8}
{Station Latitude}{40.5030}
{Station Longitude}{-124.0990}
{File Name (Horizontal 1)}{CAPEMEND/RIO270}
{File Name (Horizontal 2)}{CAPEMEND/RIO360}
{File Name (Vertical)}{CAPEMEND/RIO-UP}
{HP-H1 (Hz)}{0.070}
{HP-H2 (Hz)}{0.070}
{LP-H1 (Hz)}{23.000}
{LP-H2 (Hz)}{23.000}
{PGA (g)}{0.4244}
{PGV (cm/sec)}{47.95}
{PGD (cm)}{16.96}
